**Broomy Plain – update January 2020**

In the week beginning 27 January, work is due to start on a number of modifications to the verge restoration work at Broomy Plain.

These come following matters raised at the Verderers Court in July, which the Verderers and Forestry England are happy to address as follows:

* The remaining dragon’s teeth will be installed (in conjunction with the work referred to below) to allow a single carriageway width of 4.5m.
* Dragons’ teeth will be installed as equidistant from each side of the carriageway as possible. This may mean that some of the existing dragons’ teeth will be moved away from their current position adjacent to the grasscrete (depending on the location of any utilities and road foundations).
* The distance between dragons’ teeth will be extended (compared with the current positioning).
* The dragon’s teeth at the entrance and exit to the passing places will be removed to improve manoeuvrability to encourage vehicles to make full use of the whole of the passing place.
* Dragon’s teeth close to the chicane will be removed.
* The roadside scrub and gorse opposite the entrance to Broomy Lodge on the inside bend have already been cut to improve visibility.

Thank you for your understanding while works are carried out.  Any questions? Please email hls.enquiries@forestryengland.uk